Buzzer

Line Sensor

Brightness adjustment

Arduino Nano

Pi Camera

Li-Po Battery

11.1 V, 2200 mAh

Power Bank

Line Sensor

Pick and Place Mechanism

L298N Motor Driver

Raspberry Pi Model 3 B+

USB Power